CRUSADER 2 NOTE'S  450 PAGES
1.TO CHECK RS232 JUMPER 2-3 AND 6-20 OR FROM THE HEADER FROM LEFT TO
RIGHT JUMPER 1 & 2  THEN JUMPER 7 & 8
2.PUSH MANUAL
3.PULL ESTOP
4.AUX 2740
5.START
6.PASS = 0
7.FAIL ERRORS 38 OR 39
8.FAIL ERROR 30 = SYSTEM HAS NO RS232 SOFTWARE

TO MAKE A CABLE FOR A CRUSADER 2 
FROM DB9 FEMALE TO DB25 FEMALE
1		1
2		3
3		2
4		20
5		7
6		6
7		4
8		5
9		22


1.POWER SUPPLY CONN ON TOP OF CPU CENTER WIRE POWER FAIL = 0VDC
2.fix for rs232 1.pull out 8251 pin 19 jummper to pins 9 & 10 on 1488
 cut out u8 and jumper pins 5 & 7 and then jumper pins 9 & 11
*******************************************************************

ANILAM CRUSADER M CRT
1.IC1 AN5430 PANASONIC

2.Error code 9001= bad cpu 


